**302-1 Pavement Pulverization (Revised 2-27-14 M)**

**(Revise for each Project)**

1. PAVEMENT PULVERIZATION [302] (REVISED 2-27-14 M)

Process the existing plant mix surfacing with existing crushed aggregate course, additional crushed aggregate course, or combination of these to restore the roadway section meeting the requirements of Section 302 and this provision.

Uniformly blend the pulverized plant mix surfacing, existing base course, crushed aggregate course, or combination of these to assure a maximum 50 percent pulverized plant mix surfacing throughout the blend material sections. The existing plant mix depths on the project are as follows:

| From | To | Average Width | Depth |
| --- | --- | --- | --- |
| Station. | Station. | Width | Depth |
| Station | Station. | Width. | Depth |