1. COLD MILLING [411] (ADDED 10-11-12)

After cold milling, do not leave the remaining pavement exposed to traffic more than 24 hours before placing the plant mix surfacing.