1. PERMANENT EROSION CONTROL GEOTEXTILE (revised 2-2-2022)

Description. Provide Non-Woven Permanent Erosion Control Geotextile, High Survivability, Class B, meeting the requirements of Section 716. The geotextile under the Class 3 Riprap must have a minimum mass per unit area of 16 oz./sq. yard in accordance with ASTM D5261.