1. SPECIAL BACKFILL FOR CULVERTs (revised 2-2-2022)

Description. Place special backfill at the locations shown on the project plans and cross sections. Place special backfill to the bottom of the crushed aggregate course section or as shown in the plans.

Materials. Provide backfill material consisting of Crushed Aggregate Course (CAC).

Construction. Compact Special Backfill in accordance with Section 203, limiting the lift thickness to 6 inches.

Method of Measurement. Special Backfill is measured by the cubic yard in place.

Basis of Payment. Special Backfill is paid at the contract unit price bid per cubic yard complete and in place.