1. ROD SOUNDINGS - SPREAD FOOTINGS (Revised 5-29-03)

Description. Excavate for bents that have multiple individual substructure units so that the rod soundings for the separate footings all get submitted at the same time for approval of footing elevations.

Basis of Payment. No separate payment for this work is allowed as the work is considered incidental to the completion of other work.