1. speed feedback sign size [618] (added 8-28-25)

Rescind Subsection 618.03.10 (A) and replace it with the following:

Furnish a Speed Feedback Sign (SFS) with a static sign measuring a minimum size of 36” x 48”.